**Pool Testing Directions**

**Kit and Charts in baby pool gate (TUC)**

Fill sample device

At least 12” below surface on big pool

Approximately midway down on baby pool

**Free Chlorine**

Fill small tube

Add 5 drops of R-0001

Add 5 drops 0f R-0002

Mix and Read

**Total Chlorine (don’t have to do)**

Add 5 drops of R-0003

Mix and Read

**PH**

Fill Large (44ml) tube

Add 5 drops of R-0004

Mix and Read

**Total Alkaline**

Fill large tube to 25 ml (1/2 way full)

Add 2 drops of R-0007

Swirl to mix

Add 5 drops of R-0008

Swirl to mix

Add drops of R-0009

Swirl to mix after each drop until it turns pink

Sample turns pink

Record as 10 times number of drops

**Pool Committee Responsibilities**

* Test water with chemicals Saturday and Sunday. Record findings in log.
* Clean skimmers
* Skim water surface if necessary
* Line up all chairs and loungers with top edge down. All umbrellas should be down and secured when not in use
* Clean up any garbage left on deck or tables.
* Add water to pool if water level lowers below skimmers
* Make sure green light is on in pump room to show phone is working.
* Take out garbage on Tuesday night.
* Enforce all rules of the pool with users when necessary.
* Make sure all gates are locked and secure.
* Sweep deck as needed
* Check restrooms to make sure there are no issues, install toilet paper as needed. Turn off lights.
* If you find anything suspicious, potential safety problem, or something you do not understand please report it.